|  |  |  |
| --- | --- | --- |
| Product Condensate Pumps  CP Series Condensate Pumps  Application Condensate removal for HVAC/R equipment  Purpose This product Is designed to automatically evacuate condensate or water discharge from HVACR equipment up to 22' vertically once the condensate in the reservoir reaches a speci­fied level.  Advantages AsurityTM CP-22 series pumps beat the industry standard of 20’ lift height by 2 feet and come with innovative features such as: vibration dampening feet and motor mounts, metal mounting tabs, four inlet holes (and 3 poly covers for the unused), LED indicators, float switch and duckbill-style check valve, and detailed installation instructions. Two terminals are provided allowing the installer flexibility to connect air-handler shut-down, an important safety consideration. CP-22 is available with 20’ of 3/8” tubing as well.  Utilizing the same great features but in a low-height (4-3/8”) design, the CP-22LP is great for tight spaces.  Maximum Condensate Temperatures   * Continuous duty 140°F * Maximum inlet temperature 160°F * Not suitable for contact with steam or gases that exceed 160°F   Rated Voltage 120VAC / 230VAC / 60hHz  Rated Current Draw   * 1.9 Amps (120VAC) * 1.0 Amps (230VAC)   Input Type   * USA 3-prong molded plug (120VAC) * NEMA 6-15 (230VAC)   Maximum Lift Height   * CP-22 series: 22’   (Every AsurityTM condensate pump is computer tested to ensure excellent performance at all pumping levels.)  Included Accessories   * Instruction Booklet * Metal Hang Tabs (plastic on CP-16) * 4’ Remote Shutoff Leads w/insulated terminals * Polyethelene inlet covers (3)   Wiring Color References   * 120V   - Black – Live/Hot  - White – Neutral  - Green – Ground  - (All installations must conform to local building codes)   * 230V   - Brown – Live/Hot  - Blue – Live/Hot  - Green/Yellow – Ground - (All installations must conform to local building codes) | Flow Rate @ Zero Head   * CP-22: 1.6 gallons per minute   Dimensions   * CP-22: 11.8” x 5.9” x 6.7” (4.9” low profile) * CP-22: 5 lbs. (4.7 lbs. low profile)   Inlet Height from Base   * CP-22: 4.4” (1.75” low profile)   Tank Capacity   * CP-22: 1/2 gallon * CP-22LP: 3/8 gallon | |
| SKU Specific Package Metrics   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **CATALOG NO.** | **DESCRIPTION** | **LIFT** | **UPC** | **ORDER MULTIPLE** | | CP-22 | 120V | 22’ | 095247091263 | 6 | | CP-22T | 120V w/ tubing | 22’ | 095247091287 | 6 | | CP-22-230 | 230V | 22’ | 095247092994 | 6 | | CP-22-230T | 230V w/ tubing | 22’ | 095247094578 | 6 | | CP-22LP | 120V low profile | 22’ | 095247094301 | 6 | | CP-22LP-230 | 230V low profile | 22’ | 095247131280 | 6 |   CP-22 Pump Performance Curve  Chart, line chart  Description automatically generated | |