|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Product CP-M115/M230  Low Profile, Mini-Split Pump CP-M115, CP-M230  Features   * Compact Size * Flexible installation options. Fits inside line set covers or inside cassette * Clear Reservoir * Dual Outlet Reservoir * Reservoir Mounting Plate * Up to 6’ Suction Lift - 24’ Total Lift * For systems up to 2.8 tons (34,000 BTUs – 10kW) * Quiet. < 21dB(A) * Thermally Protected * Built-In Overflow Switch – SPDT Alarm Circuit * 2 Year Warranty * ETL Listed * Water Resistant Sensor Cable   Specifications   |  |  | | --- | --- | | **Voltage** | 110 – 120VAC or 220 – 240VAC | | Hz | 50/60Hz | | Watts | 19W | | IP | IP64 | | Duty Cycle Rating | 70% | | Sound | <21 dB(A) at 3.3’ | | Overflow Switch | 5A @ 250VAC Resistive | | Working Temperature | 41ºF to 113ºF (5ºC to 45ºC) | | Storage Temperature | 37ºF to 158ºF (3ºC to 70ºC) | | ETL | 4000786 (Conforms to UL STD 778) | | CSA | C22.2 NO. 108 |   UPC   |  |  | | --- | --- | | CP-M230 | 0095247152759 | | CSA | 0095247152742 | |  | |
|  | |