1. Format a USB Flash drive in Fat32
2. Copy install.img from the downloaded folder to the root directory (the parent/top directory) of the USB flash drive.
3. Ensure the WIFI2HDMC is powered off.
4. Plug the USB flash drive into the USB Media Input on the WIFI2HDMC.
5. Hold down the mode select button and turn on the WIFI2HDMC by pressing the power button. Continue to hold down the mode select button while the device powers on.
6. Release the mode select button after the “Please wait for USB update” appears on your HDMI-enabled display device.
7. The firmware on your WIFI2HDMC will now update. Once the update has completed the new primary launch page will be displayed