,z_Speaker Side Distance 2##LENGTH##INCHES,Width##LENGTH##INCHES,Height##LENGTH##INCHES,Depth##LENGTH##INCHES,Product data url##OTHER##,Product Page URL##OTHER##,Product Material##OTHER##,Material Note##OTHER##,Model##OTHER##,Description##OTHER##,Frequency Range##OTHER##,Electrical Power Requirements##OTHER##
SA101-SUB - Custom,6,12,34,5.38,,https://www.jamesloudspeaker.com/products/13,Sonance - Metal - Aluminium,Contact MFR for more info,SA101-SUB,"3"" (minimum) Grille Small Aperture® Subwoofer",33Hz-150Hz ± 3dB,100-350W
SA101-SUB - Black,6,12,34,5.38,,https://www.jamesloudspeaker.com/products/13,Sonance - Metal - Black,,SA101-SUB,"3"" (minimum) Grille Small Aperture® Subwoofer",33Hz-150Hz ± 3dB,100-350W
SA101-SUB - White,6,12,34,5.38,,https://www.jamesloudspeaker.com/products/13,Sonance - Metal - White,,SA101-SUB,"3"" (minimum) Grille Small Aperture® Subwoofer",33Hz-150Hz ± 3dB,100-350W
SA81-9-SUB - Custom,5,10,18,9,,https://www.jamesloudspeaker.com/products/588,Sonance - Metal - Aluminium,Contact MFR for more info,SA81-9-SUB,Small Aperture Ceiling Subwoofer,37Hz-120Hz ± 3dB,100-300W
SA81-9-SUB - Black,5,10,18,9,,https://www.jamesloudspeaker.com/products/588,Sonance - Metal - Black,,SA81-9-SUB,Small Aperture Ceiling Subwoofer,37Hz-120Hz ± 3dB,100-300W
SA81-9-SUB - White,5,10,18,9,,https://www.jamesloudspeaker.com/products/588,Sonance - Metal - White,,SA81-9-SUB,Small Aperture Ceiling Subwoofer,37Hz-120Hz ± 3dB,100-300W
SA54-4-SUB - Custom,7,14,32,3.4,,https://www.jamesloudspeaker.com/products/49,Sonance - Metal - Aluminium,Contact MFR for more info,SA54-4-SUB,"3"" (minimum) Grille Small Aperture® Ultra-Slim Subwoofer",38Hz-150Hz ± 3dB,75-250W
SA54-4-SUB - Black,7,14,32,3.4,,https://www.jamesloudspeaker.com/products/49,Sonance - Metal - Black,,SA54-4-SUB,"3"" (minimum) Grille Small Aperture® Ultra-Slim Subwoofer",38Hz-150Hz ± 3dB,75-250W
SA54-4-SUB - White,7,14,32,3.4,,https://www.jamesloudspeaker.com/products/49,Sonance - Metal - White,,SA54-4-SUB,"3"" (minimum) Grille Small Aperture® Ultra-Slim Subwoofer",38Hz-150Hz ± 3dB,75-250W
