Support OS:
SuSE Linux Enterprise Desktop 10 32bit
SuSE Linux Enterprise Server 10 32bit

Support Chip/Mode:
JMB360/1/2/3/5/6/8 IDE mode
JMB360/1/2/3/5/6 AHCI mode

Steps:
1. Use dd(Linux) or Rawritewin.exe(Windows) to write driver disk.
2. Make sure your JMB36x is set in IDE or AHCI mode.
3. CD/DVD boot form OS installation disc.
4. Insert driver disk to floppy drive.
5. Select "Installation" and fill in "Boot Options" with "manual=1".
6. Select the language.
7. Choose a keyboard map.
8. Select "Kernel Modules (Hardware Drivers)"
8-1. If you are using USB Floppy drive, please select "usb-storage" module first.
9. Select "Add Driver Update" and exit to Main Menu.
10.Start Installation or System -> Start Installation or Update
11.Install OS in the normal process.

Known Issues:
None

MD5SUM
6f776ab65cb2ebb7c60c22e0f8b85b23	sle10.img