


P/N: 19252-100
FLIR IRW-4C: 4in Round Infrared Inspection Window (Aluminum)
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	General description

	This device is a viewport which consist of a crystal "glass" window, mounted in an aluminum frame. The glass is specially formulated to allow transmission of infrared light to allow use of infrared thermal sensing equipment without opening the enclosure. This device is intended for installation in doors or walls of electrical enclosures without compromising the integrity of the enclosure.

	Power system

	Voltage
	Any range



	Environmental data

	Environment
	Indoor/outdoor type 4/12

	Operating temperature range
	Maximum: 260°C (500°F)

	Storage temperature range
	Optics, maximum: 1357°C (2474°F)

	Physical data

	Size (L × W × H)
	29.3 × 127 × 137 mm (1.15 × 5.01 × 5.37 in.)

	Viewing aperture diameter
	89 mm (3.50 in.)

	Material
	Optics: CaF2 (Calcium Fluoride Crystal)
Body: Anodized aluminum
Hardware: steel

	Comments to physical data
	Required hole diameter, nominal: 114.3 mm (4.5 in.)
Greenlee Punch: 742BB
Maximum pullout strength: 1678 kg (3700 lb.)



	Lens

	Waveband
	Broadband IR: short-, mid-, and longwave

	Visible light spectrum
	Yes

	Certifications

	Certification
	UL, IP67, NEMA Type 4/12, CSA



	Shipping information

	Packaging, type
	Cardboard box

	List of contents
	· IR window
· Case
· Mounting instruction
· Additional safety screw

	Packaging, weight
	0.46 kg (1.01 lb.)

	Packaging, size
	165 × 175 × 40 mm (6.50 × 6.89 × 1.58 in.)

	EAN-13
	4743254000742

	UPC-12
	845188002831

	Country of origin
	Estonia
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