This version of the driver supports all the Novell frame types.



Supported keywords.

A keyword has been added to allow the user to configure the line speed.

The format is: CONTYPE <number>.

By specifying a number (described below) the linespeed can be configured.
The recommended setting is 1/AUTO, where the driver will use autonegotiation
to determine the linespeed.

The follow values are defined for parameter CONTYPE
1   AUTO
2   1000MB
3   100MB Full duplex
4   100MB Half duplex
5   10MB Full duplex
6   10MB Half duplex

When the keyword is not specified, the driver will default to AUTO.
