Please note: For all normal use cases please use the Win X,X driver installs. 

The driver labeled Win 10_11_11014.20_10060.20_BurstOff_Driver is specifically for use on Win 10/11 in applications where 
the setup is having issues with dropping network connection during heavy use or video calls.

This driver turns off the RTL8153 chipsets packet bursting option as a work around from Realtek. 

This driver requires the Setup.exe to be run to install correctly. 