########################################################
#              HBA Configuration.                      #
########################################################
[ADAPTER CONFIG]       #adapter config
[BEGIN]

#[VDNAME]="Marvell RAID"
#[VDNAME]="MRVL RAID_"

[MAX_PORT_NUMBER]=8
#[FRONTEND_P0]=FFFFFFFF
#[FRONTEND_P1]=FFFFFFFF
#[FRONTEND_P2]=FFFFFFFF
#[FRONTEND_P3]=FFFFFFFF
#[FRONTEND_P4]=FFFFFFFF
#[FRONTEND_P5]=FFFFFFFF
#[FRONTEND_P6]=FFFFFFFF
#[FRONTEND_P7]=FFFFFFFF

#[BIOS_SHOWING_TIME]=2000 #Its unit is milli-second(0~65534). Default is 2000ms if no defined.

#[PNP_AUTO_REBUILD]=ENABLE
#[PNP_AUTO_REBUILD]=DISABLE

#[OEM_RAID_CFG_VD0]=00000F00 #configure VD0: bit31~bit28:Reserved, bit27~bit8:port mapping bit(the example is setting the port3,2,1,0), bit7~bit0:Raid type(the example is RAID0)

#[BUZZER]=ENABLE
#[BUZZER]=DISABLE

#[SPINUP GROUP]=1 #SPIN_UP 4 ~ 1 devices together(0:no waiting). FF:Disable
#[SPINUP TIME]=5 #wait 30 ~ 1 seconds to wake up next device(0:no waiting). FF:Disable

#[SMART_CHECK]=ENABLE
#[HALT_ON_ERROR]=ENABLE

[UPGRADE_FW]=ENABLE
#[UPGRADE_FW]=DISABLE

[INT13]=ENABLE
[INTELLIGENT]=DISABLE
#[INTELLIGENT]=ENABLE
[CTL_GPIO_LED]=DISABLE
#[CTL_GPIO_LED]=ENABLE

[AES]=DISABLE
#[AES]=ENABLE
#[AES_OS_BOOTING]=ENABLE

[FREE_DISK]=ENABLE
#[FREE_DISK]=DISABLE
#[RAID0_MIGRATE_RAID1]=ENABLE
#[RAID0_MIGRATE_RAID1]=DISABLE
[RAID FEATURE]=ENABLE
#[RAID FEATURE]=DISABLE
[RAID0]=ENABLE
#[RAID0]=DISABLE
[RAID1]=ENABLE
#[RAID1]=DISABLE
[RAID10]=ENABLE
#[RAID10]=DISABLE
[HyperDuo_CAPACITY]=ENABLE
#[HyperDuo_CAPACITY]=DISABLE
[HyperDuo_SAFE]=ENABLE
#[HyperDuo_SAFE]=DISABLE
#[HYPERDUO_HYBRID]=ENABLE
[HYPERDUO_HYBRID]=DISABLE
[INT13VISIBLE]=DISABLE
[P0_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P1_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P2_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P3_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P0_PHY_TUNNING_1]=FFFFFFFF
[P0_PHY_TUNNING_2]=FFFFFFFF
[P0_PHY_TUNNING_3]=FFFFFFFF
[P1_PHY_TUNNING_1]=FFFFFFFF
[P1_PHY_TUNNING_2]=FFFFFFFF
[P1_PHY_TUNNING_3]=FFFFFFFF
#[P2_PHY_TUNNING_1]=FFFFFFFF
#[P2_PHY_TUNNING_2]=FFFFFFFF
#[P2_PHY_TUNNING_3]=FFFFFFFF
#[P3_PHY_TUNNING_1]=FFFFFFFF
#[P3_PHY_TUNNING_2]=FFFFFFFF
#[P3_PHY_TUNNING_3]=FFFFFFFF
[END]
