#CPU AHCI 9230
{0xD0060018,[0xA21E4000]}, #MBUS Address Remap Control 2, offset 0x1E4000
{0xD0060020,[0x00001F00]}, #Remap Size Control, Extend to 2048K
{0xD0040828,[0x06010000]}, #Expansion-Rom SPI access base address
{0xD0030030,[0x0003FFFF]}, #Entend to 256K
{0xD004081C,[0x00015038]}, #6G drives issue/Disable HW CC
{0xD004080C,[0xA5A58757]}, #SSC parameter calculate in PLL CTL2
{0xD0040808,[0x0001388F]}, #SSC parameter calculate in PLL CTL1
{0xD0040800,[0x17FD0988]}, #PAD and Voltage regulator control
{0xD0040820,[0x44444444]}, #Memory timing control RTC = 00 
{0xD0040824,[0x10444444]}, #LUNIT memory timing control RTC = 00
{0xD0030000,[0x92301B4B]}, #Device ID and Vendor ID
{0xD003002C,[0x92301B4B]}, #SubDevice ID and SubVendor ID
{0xD0032008,[0x00000006]}, #flip the PCIE retry
{0xFFFFFFFF,[0x02002009]}, #Version
{0xFFFFFFFF,[0xFFFFFFFF]};
