########################################################
#              HBA Configuration.                      #
########################################################
[ADAPTER CONFIG]       #adapter config
[BEGIN]

#[SPINUP GROUP]=1 #SPIN_UP 4 ~ 1 devices together(0:no waiting). FF:Disable
#[SPINUP TIME]=3 #wait 30 ~ 1 seconds to wake up next device(0:no waiting). FF:Disable

#[BIOS_SHOWING_TIME]=3000 #Its unit is milli-second(0~65534). Default is 2000ms if no defined.

#[BIOS_SCANING_DIRECT]=ENABLE #Detecting direction change for BIOS dual controllers.

#[BIOS_INITIALING_STR]=ENABLE #That will show the initialling string in screen, replace black screen.

#[SMART_CHECK]=ENABLE
#[HALT_ON_ERROR]=ENABLE

[P0_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P1_RATE]=6Gb/s        #1.5Gb/s or 3Gb/s or 6Gb/s
[P0_PHY_TUNNING_1]=FFFFFFFF
[P1_PHY_TUNNING_1]=FFFFFFFF
[P0_PHY_TUNNING_2]=FFFFFFFF
[P1_PHY_TUNNING_2]=FFFFFFFF
[P0_PHY_TUNNING_3]=FFFFFFFF
[P1_PHY_TUNNING_3]=FFFFFFFF
[END]
