
Version 1.0.0.5
-------------------------------------
It supports all possible combination/modes of MCS9845 like:
0P1S,0P2S,0P4S,0P6S,1P0S,1P1S,1P2S,1P4S,2P0S,2P1S,2P2S.


Version 1.0.0.4(Custom Release)
-------------------------------------
1)Custom Release  support the 8 bytes of Rx fifo trigger level

Version 1.0.0.4
------------------
-Added Parallel port support and supports mode 4S1P



Version 1.0.0.3
------------------
1)Fixed the Bug id:5424 and 5413
2)Description:
Bug id:5424=>Lost of characters during file transmission from XP to CE device.
Bug id:5413=>While tranmitting "data" from CE to XP device,the very first character we get on XP device is junk
	     followed by data.