Version 1.0.0.5
-------------------------------------
It supports all possible combination/modes of MCS9845 like:
0P1S,0P2S,0P4S,0P6S,1P0S,1P1S,1P2S,1P4S,2P0S,2P1S,2P2S.


Version 1.0.0.4
----------------
As we have used the source of "Version1.0.0.4" of "WinCE 5.0 9845" driver,so the 
version for WinCE6.0 driver is "Version1.0.0.4"