NETWARE README.TXT FOR NETWARE 3.1X, 4.1X AND 5.0
---------------------------------------------------------------
ALL VERSIONS

When the HAM driver is loaded the banner will indicate that
the driver is for Netware 4.11. This driver, however, will
function properly  under Netware 3.1X and 4.1X. Please follow
the version specific installation instruction below to 
properly install the Netware driver.

NETWARE 3.1X

To use the INIA100U2W under NetWare 3.1x the system must be 
upgraded to use the NetWarePeripheral Architecture (NWPA). 
The upgrade package, NWPA_UP.EXE, can be downloaded 
from Novell's web site at 
www.developer.novell.com/devres/sas/certinfo.htm


Before running the installation routine:

1.  Create the directory SERVER.312

2.  Copy NWPA_UP.EXE to C:\SERVER.312

3.  Execute NWPA_UP.EXE in C:\SERVER.312 directory

4.  Delete NBI.NLM and NWTAPE.CDM

5.  Execute 312PTC.EXE in the same directory

6.  Create the directory C:\SERVER.312\CDSAVE

7.  Copy CDROM.NLM to C:\SERVER.312\CDSAVE

8.  Copy INIA100.HAM and INIA100.DDI to the SERVER.312 directory

NEW NETWARE 3.1X INSTALLATION

9.  Change to the NETWARE\ENGLISH directory on the installation CD

10. Enter INSTALL begin the installation routine

11. At the server console enter the following commands
	LOAD 312PTC\NATIVE\START\NPAPATCH
	LOAD MMATTRFX
	LOAD NBI31X

12. Load the INIA100.HAM driver LOAD C:\SERVER.312\INIA100.HAM

13. Continue the installation by loading INSTALL.NLM creating 
    partitions and volumes

14. Create STARTUP.NCF file

15. Create the AUTOEXEC.NCF file and add the following lines 
    before saving
	LOAD AFTER311
	LOAD C:\SERVER.312\MMATRFX
	LOAD C:\SERVER.312\NWPALOAD
	SEARCH ADD 1 C:\SERVER.312\CDSAVE
	LOAD CDROM

16. At the server console enter the following command
	LOAD C:\SERVER.312\PATCH312

17. Down and reboot the server

CURRENTLY INSTALLED 3.12 SERVER

9. Edit the STARTUP.NCF file and add the following lines after any 
   set parameter but before any file loading
	LOAD C:\SERVER.312\312PTC\NATIVE\START\NPAPATCH
	LOAD C:\SERVER.312\MMATTRFX
	LOAD C:\SERVER.312\NBI31X

10. Boot the server, dismount any CD-ROM volumes if mounted, 
    unload CDROM.NLM if loaded then load INSTALL.NLM

11. Edit the AUTOEXEC.NCF and replace the line that loads 
    CDROM.NLM with the following lines
	LOAD AFTER311
	LOAD C:\SERVER.312\MMATTRFX
	LOAD C:\SERVER.312\NWPALOAD
	SARCH ADD 1 C:\SERVER.312\CDSAVE
	LOAD CDROM

12. Down and exit the server, the reboot

-----------------------------------------------------------
NETWARE 4.1X

To use the INIA100U2W under NetWare 4.1x the system must be 
upgraded to use the latest NetWare Peripheral Architecture 
(NWPA) The upgrade package, NWPA_UP.EXE, can be downloaded 
from Novell's web site at 
www.developer.novell.com/devres/sas/certinfo.htm

1.  Create the directory C:\UPDATE

2.  Copy NWPA_UP.EXE to C:\update

3.  Copy INIA100.HAM and INIA100.DDI to C:\UPDATE

4.  Execute NWPA_UP.EXE in the C:\UPDATE directory

5.  Delete NBI31X.NLM, NWTAPE.CDM and NWTAPE.DDI

NEW NETWARE 4.11 INSTALLATION

6.  Begin the installation routine (INSTALL.BAT on the root of 
    the install CD)

7.  When prompted to edit e STARTUP.NCF file by placing the 
    following line after any set parameter but before any file
    loading
	LOAD C:\NWSERVER\UPDATE\NWPA
	LOAD C:\NWSERVER\NBI

8.  When prompted to select a device driver to load, select 
    INIA100.HAM from the 
    C:\UPDATE directory

9.  Continue installation

10. When prompted to add any lines to the AUTOEXEC.NCF file add
    the following lines
	LOAD C:\UPDATE\CDROM

11. Down and exit he server

CURRENTLY INSTALLED 4.11 SERVER

6. From DOS edit the STARTUP.NCF file and add the following lines 
   after any set parameters but before any file loading
	LOAD C:\UPDATE\NWPA
	LOAD C:\UPDATE\NBI
	LOAD C:\UPDATE\INIA100.HAM

7. Boot the server and dismount any CD-ROM volumes if mounted and 
   unload CDROM.NLM if loaded

8. Edit the AUTOEXEC.NCF file and replace the line to load
   CDROM.NLM with the following line, and save the file
	LOAD C:\UPDATE\CDROM

9. Down the server and reboot

----------------------------------------------------------------
NETWARE 5.0

NEW NETWARE 5.0 INSTALATION

1.  Begin the install routine (INSTALL.BAT from the root of the 
    installation CD)

2.  At the screen listing detected device drivers select MODIFY

3.  Select STORAGE ADAPTERS and press ENTER

4.  Delete INI9100.HAM

5.  Press INS twice followed by F3 to add a driver

6.  Place the INI-A100U2W driver diskette into the floppy drive 
    and press enter

7.  At the next screen select RETURN TO DRIVER SUMMARY

8.  Continue the installation as described in the User's Manual.



