Initio INI-A100U2W Device Driver for Windows 2000
------------------------------------------------------------------

Index

1) Initio Technical Support
2) Diskette Contents
3) Windows 2000 INSTALLATION


1)  Initio Technical Support
--------------------------------------

Initio Corpration
2205-A Fortune Drive
San Jose, CA 95131

(408) 965-5039 -- Tech Support
(408) 577-0640 -- FAX
support@initio.com
http:\\www.initio.com


2)  Diskette Contents
------------------------------

 +--ROOT
 |  |
 |  +--README.TXT      : This file.
 |  +--TXTSETUP.OEM    : OEM script file for Windows 2000.
 |  +--INIA100.INF     : OEM script file for Windows 2000.
 |  +--DISK1           : script file for Windows 2000.
 |
 +--WIN2K
    |
    +--INIA100.SYS     : Device Driver(v1.01) for WINDOWS 2000.
  

3) Windows 2000 INSTALLATION
------------------------------------------------

 Adding or Updating the Initio driver to an existing Windows 2000 system
 booted from an IDE drive or different type of host adapter:

Install the A100U2W in an open PCI slot, do not attach any cables to the adapter.

     1. Establish a Win2000 session.
         Select CONTROL PANEL from within the MY COMPUTER group.
         Select ADD/REMOVE  HARDWARE  from within the CONTROL PANEL group,
         Click on NEXT.

     2. Windows will show the Hardware Wizard and ask you to click on NEXT.
         Select ADD/TROUBLESHOOT A DEVICE, then click on NEXT.
         Select ADD A NEW DEVICE, then click on NEXT.

     3. Windows will now ask you to choose either SEARCH FOR NEW HARDWARE  or
         to SELECT THE HARDWARE FROM A LIST. You want to SELECT THE HARDWARE
         FROM A LIST, then click on NEXT.

     4. Select SCSI and RAID CONTROLLERS, click on NEXT. 
         Select the HAVE DISK option and point Windows to the drivers (either on
         the floppy disk or the temp directory where you unzipped the drivers).
         The Initio INI-A100U2W PCI SCSI Controller should be listed on the 
         screen, Highlight it and click on NEXT.  You may need to click on NEXT
         at a couple of more screens until Windows comes up with a warning
         about the driver not being tested for Windows 2000, at this point it
         will ask if you wish to continue, click on YES then click on FINISH at
         the next screen. 

This should successfully install the drivers, in which case you can now shutdown
the machine and connect your devices to the A100U2W and reboot.


 Floppyless SETUP
 --------------------------
      If you are running WINNT.EXE or WINNT32.EXE to install or upgrade 
      Win2000, when system reboots and the screen turns black with the text 
      "Setup is inspecting your computer's hardware configurartion...",
      You have two seconds to press the  'F6' key to enter the DRIVER INSTALL 
      SCREEN, this is the time to insert the Initio driver diskette and
       type "A:\WIN2K" to load the INI-A100U2W Win2000 driver.

