


    /*******************************************************************
    *                   Initio INI-A100U2W                             *
    *                  Windows 95 device driver                        *
    ********************************************************************/

   FILES YOU NEED:
   -------------------------------------------------------------------------
      Information script files for installation: INIA100.INF.
      Miniport device driver: INIA100.MPD.

   INSTALLATION:
   -------------------------------------------------------------------------
   A: New Windows 95 installation:
   B. Adding INI-A100U2W to an existing Windows 95:
   C. Updating device driver:


   A: New Windows 95 installation:
         =============================

         1. Run SETUP.EXE from the Windows 95 CD-ROM and follow the direction
            on your screen.

         2. After a Windows 95 session is established, 
            select "My Computer/Control Panel/System/Device Manager/Other-
            devices/PCI SCSI Bus Controller" from the Windows 95 desktop.

         3. Click the "Driver" tab, then click the "Change Driver" tab.

         4. Double click "SCSI controllers", then click the "Have Disk" button.

         5. At the prompt, type in "A:\win95", insert Initio INI-A100U2W
            driver disk 1, and click the "OK" button. 
      

         6. Select "Initio INI-A100U2W Host Adapter", click the "OK" button.
            Windows 95 will copy INIA100.MPD to your hard disk. Reboot to complete
            the driver installation.



   B. Adding INI-A100U2W to an existing Windows 95:
         ================================================

         1. Install the Initio hardware as described in the User Manual/User Guide.
            Windows 95 will detect the presence of a new hardware.

         2. When Windows 95 displays the following:
         +----------------------------------------------------------------+
         |  New Hardware Found                                            |
         |  PCI SCSI Bus Controller                                       |
         |  Select which driver you want to install for your new hardware:|
         |  * Driver from disk provided by hardware manufacture           |
         |  OK   Cancel   Help                                            |
         +----------------------------------------------------------------+
                 Click "OK".

         3. Windows 95 will then display the following:
         +----------------------------------------------------------------+
         |  Install From Disk                                             |
         |  Insert the manufactures's installation disk into the drive    |
         |  selected, and then click OK                                   |
         |  Copy manufacturer's files from                                |
         |  A:\WIN95                                                      |
         +----------------------------------------------------------------+
                Insert the Initio disk 1 into drive A: and Click "OK".

                WIndows 95 will interpret INIA100.INF script files and load
                INIA100.MPD driver to win95/system/iosubsys directory.
            

         4. Windows 95 will then display the following:
         +-----------------------------------------------------------------+
         |  System Settings Changed                                        |
         |  To finish setting up your new hardware, you must restart your  |
         |  computer.                                                      |
         |  Do you want to restart your computer now ?                     |
         |  Yes    No                                                      |
         +-----------------------------------------------------------------+
                Remove the diskette from drive A: and Click "Yes".

   C. Updating device driver:
         =============================

         1. From the Windows 95 desktop, select "My Computer/Control Panel/System
            /Device Manager/SCSI Controller/Initio INI-A100U2W Host Adapter".

         2. Click "Driver" tab, and then click "Change Driver" tab.

         3. Type "A:\win95" and insert Initio INI-A100U2W driver disk into floppy
            drive A:, click "OK", Windows 95 will copy the new device driver
            into your hard disk.


