
   Initio INI-A100U2W Device Driver(V1.00) for OS/2 3.X & 4.X

I)  Installation procedures for INI-A100u2W OS/2 3.X & 4.X device driver:

    i)  installed as a secondary controller
	1) Open the OS/2 System Folder.
	2) Open the System Setup Folder.
	3) Double-click "Device Driver Install".
	4) Insert the Initio installation diskette into your floppy drive.
	5) Change to the OS/2 directory.
        6) Choose INIA100.ADD, then click INSTALL.
	7) After the installation is done, OS/2 will report the status.

    ii) installed as a primary controller
	1) Make backup copies of the OS/2 Diskette 1.
        2) Copy the INIA100.ADD onto OS/2 Diskette 1.
	3) Modify the config.sys file on Diskette 1 to add
                BASEDEV=INIA100.ADD /V
	4) Install OS/2 using the backup Diskette 1
					    
 
II) Driver configuration options:

    /V          Verbose mode provides detail information about driver when
		driver is initialized
    /!V         Non Verbose mode (default)
    /ET         Driver assumes that all targets have more than one LUN (default)
    /!ET        Driver assumes that all targets only have LUN 0
    /Q:x        Specifies maximum number of tag commands per target
    /!Q         No tag command
    /B:(d,dd),. Scan devices only on PCI BUS d, DEVICE dd
    /B:d        Scan all the devices on the PCI BUS d
    /T:xxxx     Target enable mask WORD (Default scan all targets)

    /A:d        Adapter IDs are assigned based on BIOS address and
				then PCI device address
    /DM:d,..    Enable direct access storage device (DASD) support on target d
    /!DM:d,..   Disable DASD manager support on target d
    /SM:d,..    Enable SCSI manager support on target d
    /!SM:d,..   Disable SCSI manager support on target d
