Caldera OpenLinux 2.2 Installation Proceedures

This readme.txt file outlines the installation proceedure needed to install 
Caldera 2.2 on a system using an Initio SCSI adapter. You will be required 
to create a floppy disk from the files included in this package. Please format
a blank floppy with your current operating system (it does not matter which 
OS) then go to the command prompt and switch to the directory that you unzipped
this package to. You should see three files initio.img, fcopy.exe and readme.txt.

Put the formatted floppy in the drive and enter the following command:

	fcopy /Finitio.img a:  

This will create the support disk that is needed for the installation.

Next you want to insert the Caldera boot floppy in the drive and reboot the machine, 
as the machine is booting up you will see a LILO prompt at the beginning, you must 
press SHIFT and the ? keys at this prompt immeditatly. If you are successful you 
will be given a Boot:  prompt at which you enter

	install insmod=initio		(if you have the INI-9XXX series adapter)  or
	install insmod=A100U2W	(if you have the INI-A100U2W adapter)

The kernel will then be loaded from the Caldera boot floppy, as soon as it is done it 
will show a new line saying "Booting Kernel" at this prompt you have about 5 seconds 
to switch the floppy disks to the Initio floppy that you created earlier. At this point 
the installation will continue and you should have no further issues.   