The following instruction are how to install and use a Printer
connected to MosChip Parallel Port MCS7705.

1. Plug the MCS7705 in the Host Computer, a new parallel port
   will be installed in your system. You can see that under
   Device Manager, Ports.
2. Connect the Printer to USB Parallel Port. The Printer is 
   not a Plug and Play device, hence you will have to 
   manually install the printer.
3. Go to Add Printer, Select Local Printer.
4. if Windows is unable to detect a Plug and Play printer
   it will say so, Click Next Anyway.
5. Select the Printer Port, e.g if LPT2 is assigned to
   MosChip USB Parallel Port, then select LPT2. You can 
   find out the LPTx Number through Device Manager
6. Then select the Printer model and driver or enter
   the CD which contains your printer drivers.
7. Windows will install the Printer drivers and
    your Printer should be ready to use.