Firmware update for chip 88SE9128 version C0 only

Note: Program tool will have to run in DOS environment (USB or Floppy), not Windows DOS mode
1. Copy all files from the download to the root folder of the DOS Boot disk
2. Boot into DOS
3. Type “ autoexec.bat ” to start updating the firmware
4. When the screen shows "Finish !"  that means the update has completed successful.

Verify the new Firmware version:
First attach a disk to any port then power on PC and type Ctrl+M to get into the card's BIOS
Under Information check that the BIOS version is 1.1.0.1002 and Firmware Version: 2.3.0.1013