Driver extraction and installation
===================================

1. Extract the driver archive (tgz format) to a temporary folder in your datastore (ex. /vmfs/volumes/datastore1/Tehuti) by running 'tar -xvfz <driver name>.tgz
2. Verify no previous driver is installed by running the UNISTALL script. If a driver was found and removed, reboot afterwards before installing the new driver
3. When no previous driver is installed, run the script INSTALL and reboot

Driver and NIC validation
========================
1. Verify driver is installed and correct version by running 'dmesg | grep tn40'
2. Display adapters by running 'esxcfg-nics -l'
