*****************************************************************************
                               BLDSCO.TXT
*****************************************************************************
SDMS 4.0 SCO UNIX OpenServer 5

Building the SCO OpenServer BTLD Diskette

To create a BTLD diskette for SCO OpenServer 5 installations, copy the 
raw dd image file onto a 1.44 Mbytes floppy diskette. This process is 
dependent upon the operating system that you are using to create this
diskette. See the instructions below for UNIX System and DOS System Users.

*  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *

For UNIX System Users

Follow these steps to create the BTLD diskette:
 
1. Insert a 3.5" diskette into the floppy drive. 

2. At the UNIX prompt, type: 

   dd if=/<path>/sco.dd of=/dev/fd0135ds18

   The <path> is where the dd image is located. On this CD-ROM, the dd
   image file is located here:

   {UNIX CD-ROM path}/DRIVERS/UNIXES/OPNSERVR

   This command will dd the image to the floppy diskette to create a BTLD diskette.
 
*  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *

For DOS System Users

1. Use a utility that will copy the raw dd image onto a 1.44 Mbytes floppy
   diskette. RAWRITE3.COM, which is a public domain utility, is available on 
   this CD-ROM. Instructions for using this utility are included in its  
   accompanying RAWRITE3.COM file. 

2. The dd image is located here:

   {DOS CD-ROM path}:\DRIVERS\UNIXES\OPNSERVR\SCO.DD

3. RAWRITE3.COM is included on this CD-ROM at this location: 

   {DOS CD-ROM path}:\DRIVERS\UNIXES\RAWRITE3.COM

   After the image has been copied to a 3.5" floppy diskette, use this BTLD 
   diskette for SCO OpenServer installations as instructed.

  

 
