;DrIvEr DeScRiPtIoN

VER: 5.03.00
SYN: 1.00

;installation file for Symbios NWPA 1 INT/IO HAM driver: Lsi8xxNw.HAM

DR SYMBIOS_NWPA_1INT_IO_SCSI_HAM_Lsi8xxNw
{
    DES:    $Lsi8xxNw_1

    Help:   $Lsi8xxNw_2

    PAR:           2.00

;                   Bus.INC/EXC.Vendor_ID.Device_ID.Subsystem_vendor_ID.Subsystem_ID.Revision_number
    PROD:          'PCI.INCLUDE.1000.0001.*.*.*', ;53C810
                   'PCI.EXCLUDE.1000.0002.*.*.*', ;53C820
                   'PCI.INCLUDE.1000.0003.*.*.*', ;53C825
                   'PCI.INCLUDE.1000.0004.*.*.*', ;53C815
                   'PCI.EXCLUDE.1000.0005.*.*.*', ;Obsolete 53C810A
                   'PCI.INCLUDE.1000.0006.*.*.*', ;53C860
                   'PCI.EXCLUDE.1000.0007.*.*.*', ;UNASSIGNED
                   'PCI.EXCLUDE.1000.0008.*.*.*', ;UNASSIGNED
                   'PCI.EXCLUDE.1000.0009.*.*.*', ;UNASSIGNED
                   'PCI.EXCLUDE.1000.000A.*.*.*', ;UNASSIGNED
                   'PCI.EXCLUDE.1000.000B.*.*.*', ;UNASSIGNED
                   'PCI.INCLUDE.1000.000C.*.*.*', ;53C895
                   'PCI.INCLUDE.1000.000D.*.*.*', ;53C885
                   'PCI.EXCLUDE.1000.000E.*.*.*', ;Obsolete 53C825A
                   'PCI.INCLUDE.1000.000F.*.*.*'  ;53C875
;                  'Vendor_Name~Module_Name'
;                   The ";@#" is required for bacwards compatability
;@#    SPROD:      'LSI Logic~53C810',
;@#                'LSI Logic~53C820',
;@#                'LSI Logic~53C825',
;@#                'LSI Logic~53C815',
;@#                'LSI Logic~53C810A - Obsolete!',
;@#                'LSI Logic~53C860',
;@#                'LSI Logic~UNASSIGNED!',
;@#                'LSI Logic~UNASSIGNED!',
;@#                'LSI Logic~UNASSIGNED!',
;@#                'LSI Logic~UNASSIGNED!',
;@#                'LSI Logic~UNASSIGNED!',
;@#                'LSI Logic~53C895',
;@#                'LSI Logic~53C885',
;@#                'LSI Logic~53C825A - Obsolete!',
;@#                'LSI Logic~53C875'
;@#    ALIAS:      SYM8XXNW.HAM

    File:               Lsi8xxNw.HAM
    TIME:               30

    PR SLOT OPT
    {
    }

    LI Qtags OPT
    {
        DES:            $Lsi8xxNw_3

        Help:           $Lsi8xxNw_4

        CD:             $Lsi8xxNw_5
        CH:             'on'
        CD:             $Lsi8xxNw_6
        CH:             'off'
        DEF:            1
        OUT:            'qtags=%s'
    }

    PR MinTimeout OPT
    {
        DES:           $Lsi8xxNw_7

        Help:          $Lsi8xxNw_8

        TYP:           DEC (4)
        VAL:           0-1200
        DEF:           0
        OUT:           'mintimeout=%s'
    }

    LI Wide OPT
    {
        DES:            $Lsi8xxNw_11

        Help:           $Lsi8xxNw_12

        CD:             $Lsi8xxNw_13
        CH:             'on'
        CD:             $Lsi8xxNw_14
        CH:             'off'
        DEF:            1
        OUT:            'wide=%s'
    }

    PR Sync OPT
    {
        DES:           $Lsi8xxNw_15

        Help:          $Lsi8xxNw_16

        TYP:           DEC (3)
        VAL:           0,5,10,20,40,80,255
        DEF:           20
        OUT:           'sync=%s'
    }

    PR ElevatorThreshold OPT
    {
        DES:            $Lsi8xxNw_27

        Help:           $Lsi8xxNw_28

        TYP:            DEC (3)
        VAL:            0-250
        DEF:            32
        OUT:            'elev=%s'
    }

    PR NoSyncWideNegotiation OPT
    {
        DES:            $Lsi8xxNw_31

        Help:           $Lsi8xxNw_32

        TYP:            DEC (2)
        VAL:            0-99
        DEF:            99
        OUT:            'noneg=%s'
    }

    LI Verbose OPT
    {
        DES:            $Lsi8xxNw_35

        Help:           $Lsi8xxNw_36

        CD:             $Lsi8xxNw_37
        CH:             'on'
        CD:             $Lsi8xxNw_38
        CH:             'off'
        DEF:            2
        OUT:            'verbose=%s'
    }
}


DLANG:   4
;English
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   6
;French
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   7
;German
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   8
;Italian
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:    9
;Japanese
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   10
;Korean
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   12
;Portugese (Brazil)
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   13
;Russian
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   14
;Spanish
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:   16
;Chinese (Traditional)
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

LANG:    1
;Chinese (Simplified)
        $Lsi8xxNw_1="LSI Logic 8XX HAM Driver (Lsi8xxNw-5.03.00 GCA)"
        $Lsi8xxNw_2="LSI Logic NWPA SCSI Driver for NetWare 4.xx, 5.xx and 6.xx\n
            This driver should be used on machines equipped with one
            or more of the following LSI Logic SCSI chips or Host
            Adapter boards:\n
            Chips: 53C810, 53C810A, 53C815, 53C825, 53C825A, 53C860, 53C875,
            53C885, 53C895.\n
            HBAs:  SYM8100S, SYM8100ASP, SYM8150S, SYM8250S, SYM8250ASP,
                   SYM8251S, SYM8251ASP, SYM8251D, SYM8251AD, SYM8600SP,
                   SYM8751SP, SYM8751D, SYM53C895, SYM53C895A, SYM8951U.\n

            The default options are:\n
            - Tagged command queueing enabled.\n
            - Minimum timeout for SCSI devices is 0.\n
            - Support for wide devices enabled.\n
            - Support for synchronous fast-40 devices enabled.\n
            - Max supported LUNs per device = 32\n
              (when the '/lun' switch is used).\n
            - Elevator queue depth of 4.\n
            - Verbose mode is disabled.\n
            \n
            These options may be modified through the use of command line
            parameters.\n\n
            Copyright (c) 1995-2000 LSI Logic, Inc.  All rights reserved."
        $Lsi8xxNw_3 = "Tagged Command Queueing"
        $Lsi8xxNw_4 = "Tagged queueing enabled will result in the target device
                ordering commands in the queue so as to minimize actuator
                movement. This will result in a faster average I/O
                completion rate with random I/O traffic."
        $Lsi8xxNw_5 = "On"
        $Lsi8xxNw_6 = "Off"
        $Lsi8xxNw_7 = "Minimum Timeout"
        $Lsi8xxNw_8 = "Minimum Timeout setting allows 0-1200 seconds as
                a minimum timeout value before a device times out on a
                command. This is different than a default timeout which
                is a maximum timeout value."
        $Lsi8xxNw_11 = "Wide SCSI"
        $Lsi8xxNw_12 = "This option allows disabling support for wide SCSI
                processing in the driver."
        $Lsi8xxNw_13 = "On"
        $Lsi8xxNw_14 = "Off"
        $Lsi8xxNw_15 = "Synchronous SCSI"
        $Lsi8xxNw_16 = "This option allows enabling/disabling support for
                 synchronous SCSI processing in the driver. 255 says don't
                 negotiate at all."
        $Lsi8xxNw_27 = "Elevator Threshold"
        $Lsi8xxNw_28 = "The Elevator Threshold specifies the maximum number of
                requests the HAM should queue up before allowing NWPA to
                filter and organize scatter-gather request."
        $Lsi8xxNw_29 = "32 LUNs supported per SCSI device"
        $Lsi8xxNw_30 = "Allows non-zero luns to be scanned and recognized."
        $Lsi8xxNw_31 = "Disable sync/wide negotiation"
        $Lsi8xxNw_32 = "This switch disables all sync and wide negotiation for
                the specified SCSI target id. A value of 99
                indicates no selection."
        $Lsi8xxNw_35 = "Enable verbose option"
        $Lsi8xxNw_36 = "This switch instructs the driver to display
                additional driver information."
        $Lsi8xxNw_37 = "On"
        $Lsi8xxNw_38 = "Off"

;DrIvEr DeScRiPtIoN EnD
