,Description##OTHER##,Width##LENGTH##INCHES,Height##LENGTH##INCHES,Depth##LENGTH##INCHES,z_Speaker Side Distance##LENGTH##INCHES,z_Speaker Distance##LENGTH##INCHES,z_Min Support Expansion##LENGTH##INCHES,z_Max Support Expansion##LENGTH##INCHES,Product Material##OTHER##,Product Page URL##OTHER##,Model##OTHER##,Material Note##OTHER##,Electrical Power Requirements##OTHER##,Frequency Range##OTHER##
SA42-4 - White,"3"" Grille Small Aperture® Speaker",7,12,3.4,0,2.18,10,22.75,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/413,SA42-4,,25-100W,70Hz-24kHz ± 3dB
SA42-4 - Black,"3"" Grille Small Aperture® Speaker",7,12,3.4,0,2.18,10,22.75,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/413,SA42-4,,25-100W,70Hz-24kHz ± 3dB
SA42-4 - Custom,"3"" Grille Small Aperture® Speaker",7,12,3.4,0,2.18,10,22.75,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/413,SA42-4,Contact MFR for more information on Custom Colors,25-100W,70Hz-24kHz ± 3dB
SA63-4 - White,"3"" Grille Small Aperture® Speaker",11,26,3.4,0,3.5,14.5,28.25,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/63,SA63-4,,25-125W (protection limited),40Hz-22kHz ± 3dB
SA63-4 - Black,"3"" Grille Small Aperture® Speaker",11,26,3.4,0,3.5,14.5,28.25,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/63,SA63-4,,25-125W (protection limited),40Hz-22kHz ± 3dB
SA63-4 - Custom,"3"" Grille Small Aperture® Speaker",11,26,3.4,0,3.5,14.5,28.25,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/63,SA63-4,Contact MFR for more information on Custom Colors,25-125W (protection limited),40Hz-22kHz ± 3dB
SA63-7  - White,"3"" Grille High Output Small Aperture® Speaker",9.875,13.625,6.375,0,4.338,10.4,23,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/309,SA63-7,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7 - Black,"3"" Grille High Output Small Aperture® Speaker",9.875,13.625,6.375,0,4.338,10.4,23,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/309,SA63-7,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7 - Custom,"3"" Grille High Output Small Aperture® Speaker",9.875,13.625,6.375,0,4.338,10.4,23,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/309,SA63-7,Contact MFR for more information on Custom Colors,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-L  - White,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,-2.5,4.338,13.5,28.29,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/514,SA63-7-ENC-L,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-L - Black,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,-2.5,4.338,13.5,28.29,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/514,SA63-7-ENC-L,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-L - Custom,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,-2.5,4.338,13.5,28.29,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/514,SA63-7-ENC-L,Contact MFR for more information on Custom Colors,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-R  - White,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,2.5,4.338,13.5,28.29,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/515,SA63-7-ENC-R,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-R - Black,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,2.5,4.338,13.5,28.29,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/515,SA63-7-ENC-R,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-7-ENC-R - Custom,"3"" Grille, High-Output, Small Aperture® Speaker with Offset Port",9.75,13.62,6.375,2.5,4.338,13.5,28.29,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/515,SA63-7-ENC-R,Contact MFR for more information on Custom Colors,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-8  - White,6.5“ 3-Way Full-Range - 3” ceiling opening,7.75,17,7.5,0,3.775,8,16,Sonance - Metal - White,https://www.jamesloudspeaker.com/products/392,SA63-8,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-8 - Black,6.5“ 3-Way Full-Range - 3” ceiling opening,7.75,17,7.5,0,3.775,8,16,Sonance - Metal - Black,https://www.jamesloudspeaker.com/products/392,SA63-8,,25-125W (protection limited),38Hz-22kHz ± 3dB
SA63-8 - Custom,6.5“ 3-Way Full-Range - 3” ceiling opening,7.75,17,7.5,0,3.775,8,16,Sonance - Metal - Aluminium,https://www.jamesloudspeaker.com/products/392,SA63-8,Contact MFR for more information on Custom Colors,25-125W (protection limited),38Hz-22kHz ± 3dB
