,Description##OTHER##,Width##LENGTH##INCHES,Height##LENGTH##INCHES,Depth##LENGTH##INCHES,z_Speaker Side Distance##LENGTH##INCHES,z_Speaker Distance##LENGTH##INCHES,z_Min Support Expansion##LENGTH##INCHES,z_Max Support Expansion##LENGTH##INCHES,Product Page URL##OTHER##,Product Material##OTHER##,Model##OTHER##,Material Note##OTHER##,Electrical Power Requirements##OTHER##,Frequency Range##OTHER##,Impedance##OTHER##,Weight##WEIGHT##POUNDS_FORCE
SA853Q-9 - White,High Output Small Aperture Ceiling Speaker,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/517,Sonance - Metal - White,SA853Q-9,,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),34
SA853Q-9 - Black,High Output Small Aperture Ceiling Speaker,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/517,Sonance - Metal - Black,SA853Q-9,,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),34
SA853Q-9 - Custom,High Output Small Aperture Ceiling Speaker,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/517,Sonance - Metal - Aluminium,SA853Q-9,Contact MFR for more information on Custom Colors,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),34
SA853Q-6 - White,Ultra-High Output In-Ceiling Speaker for Shallow 2x6 Construction,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/593,Sonance - Metal - White,SA853Q-6,,Mid/High: 50-150W Sub: 100-300W,37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),0
SA853Q-6 - Black,Ultra-High Output In-Ceiling Speaker for Shallow 2x6 Construction,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/593,Sonance - Metal - Black,SA853Q-6,,Mid/High: 50-150W Sub: 100-300W,37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),0
SA853Q-6 - Custom,Ultra-High Output In-Ceiling Speaker for Shallow 2x6 Construction,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/593,Sonance - Metal - Aluminium,SA853Q-6,Contact MFR for more information on Custom Colors,Mid/High: 50-150W Sub: 100-300W,37Hz-20kHz ± 3dB,8 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-6 - White,Ultra-High Output,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/611,Sonance - Metal - White,SA853QT-6,,"Mid/High: 50-150W Sub: 100-300W. 	
If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-6 - Black,Ultra-High Output,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/611,Sonance - Metal - Black,SA853QT-6,,"Mid/High: 50-150W Sub: 100-300W. 	
If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-6 - Custom,Ultra-High Output,12,34,5.4,0,5.5,10,22.75,https://www.jamesloudspeaker.com/products/611,Sonance - Metal - Aluminium,SA853QT-6,Contact MFR for more information on Custom Colors,"Mid/High: 50-150W Sub: 100-300W. 	
If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-9 - White,Ultra-High Output Small Aperture Speaker with Quadratech,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/610,Sonance - Metal - White,SA853QT-9,,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-9 - Black,Ultra-High Output Small Aperture Speaker with Quadratech,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/610,Sonance - Metal - Black,SA853QT-9,,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
SA853QT-9 - Custom,Ultra-High Output Small Aperture Speaker with Quadratech,10,20,9,0,5,10,22.75,https://www.jamesloudspeaker.com/products/610,Sonance - Metal - Aluminium,SA853QT-9,Contact MFR for more information on Custom Colors,"Mid/High section 50W-150W Subwoofer section 100W-300W. If ordered as 70V, 50W mid/high, 100W subwoofer.",37Hz-20kHz ± 3dB,6 Ohms (mid/high) / 8 Ohms (sub),0
