Firmware Update Process:

Navigate to the folder labeled with the product SKU you have. Save the firmware update onto your Flash drives root folder. 
Only place the bin for your SKU on the drive. Make sure the firmware update file is un-zipped and not in a folder.
To start, press OK on “6.7 System Update” and it will automatically start updating. When
completed, turn off the system for 5 seconds and then turn back on. The firmware
update is now complete.

Release Notes:

- Improved drive compatibility.  
- Fixed issue with quick erase formatting 


