SUNIX Inc. Multi-I/O Controller Windows(R) Driver.

******************************************************************************
This driver is built for the Microsoft(R) Windows Operating Systems.

Copyright 2013 SUNIX, Inc. All names mentioned herein are a registered trademark
 or a trademark of SUNIX or its respective owners. All rights reserved.
******************************************************************************

Driver Version : 8.1.1.0

Release Data : 2013/09/13


******************************************************************************
Support platform:

  Microsoft Windows 8.1 32bit/64bit
  Microsoft Windows 8 32bit/64bit
  Microsoft Windows 7 SP1 32bit/64bit
  Microsoft Windows Vista SP2 32bit/64bit
  Microsoft Windows XP SP3 32bit/64bit

  Microsoft Windows Server 2012 R2 64bit
  Microsoft Windows Server 2012 64bit
  Microsoft Windows Server 2008 R2 SP1 64bit


******************************************************************************
DRIVER FILES:

  Setup.exe  : SUNIX Multi-I/O Controller driver package file
  readme.txt : readme text file


******************************************************************************
INSTALLATION AND REMOVAL INSTRUCTIONS:

------------------------------------------------------------------------------
Setup driver at first time
------------------------------------------------------------------------------

Step 1. Before installing the SUNIX Multi-I/O Controller Driver, press the
        [Cancel] button if Windows detect the new device.

Step 2.	Insert "SUNIX Driver" CD into the CD-ROM drive and run Setup.exe.

Step 3. Click [Next/OK] to continue the procedure.

Step 4. Press [Finish] and reboot your system to complete the installation.


------------------------------------------------------------------------------
Update driver
------------------------------------------------------------------------------

Step 1. Follow Step 2-4 described in [Setup driver at first time]
        above to complete the procedure.


------------------------------------------------------------------------------
Remove driver
------------------------------------------------------------------------------

Step 1. Go to "Start\Settings\Control Panel" and select [Add/Remove Programs]
        (or [Programs and Features]) icon.

Step 2. Select "SUNIX Multi-IO Controller" and press [Remove] button.

Step 3. Click on [Next/OK] to continue the procedure.

Step 4. Press [Finish] complete the uninstallation.

Step 5. Shutdown the system and remove hardware device to fully remove driver.


------------------------------------------------------------------------------
Silent installation
------------------------------------------------------------------------------

Run "Setup.exe /s /f2<path\logfile name>"
i.e. Setup.exe /s /f2c:\logfiledir\logfile.log


------------------------------------------------------------------------------
Silent uninstallation
------------------------------------------------------------------------------

Run "Setup.exe /s /uninst /f2<path\logfile name>"
i.e. Setup.exe /s /uninst /f2c:\logfiledir\logfile.log


******************************************************************************
RELEASE NOTE:

Ver 8.1.1.0 - 2013/09/13
    0)  release version
    1)  fix FIFO error issue for SUN2000 series
    2)  fix multiple parallel board issue for SUN2000 series
    3)  fix control sheet issue
    4)  fix a RS-422/485 issue
    5)  support Microsoft Windows 8.1 and Microsoft Windows Server 2012 R2

Ver 8.1.0.0 - 2013/03/28
    0)  release version
    1)  remove support for Windows 2000
    2)  modify port Hardware ID
    3)  modify property control sheet user interface
    4)  fix PLL function calculate error issue
    5)  fix parallel issue for SUN2000 series

Ver 8.0.0.0 - 2012/09/07
    0)  release version
    1)  support SUNIX SUN2000 products
    2)  support more languages
    3)  add PLL function
    4)  add parallel port default mode selection function
    5)  add enable legacy pnp detection setting in advanced control page
    6)  fix the printer icon lost issue in Windows 7
    7)  fix the driver crash issue when update driver
    8)  fix an issue sometimes COM port cannot access after driver installation

Ver 7.2.0.0 - 2010/12/07
    0)  release version
    1)  support internal/external GPIO
    2)  support 3-in-1 (RS-232/422/485) series
    3)  support more than three parallel ports
    4)  support SUNIX cash drawer kicker interface card
    5)  support SUNIX serial library
    6)  support multi-language UI
    7)  support silent installation
    8)  modify layout of control page
    9)  use driver dll to replace system default dll
   10)  fix an issue about H/W flow control setting in RS-422/485
   11)  fix an issue about the delay time of closing port
   12)  fix an issue about driver crash during change power state
   13)  fix an issue about buffer overflow

Ver 7.1.0.0 - 2010/01/13
    0)  release version
    1)  solve an issue about re-map series
    2)  support SUN1999 cardbus series
    3)  modify layout of control page
    4)  add reference clock setting in control page
    5)  add specific IoControl command to return part number

Ver 7.0.0.0 - 2009/07/14
    0)  release version
    1)  support Golden series, Matrix series, and SUN1999 series
